Elephant YII jekketalje 250kg

Art. Y 2 25

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Model | A | B | C | D | E | F | G | H |
| YⅡ-25 | 21 | 70 | 65 | 235 | 20 | 32 | 12 | 155 |

|  |  |  |
| --- | --- | --- |
| Model | | YⅡ-25 |
| Capacity ( ton ) | | 0.25 |
| Standard lift ( m ) | | 1.0 |
| Headroom ( mm ) | | 235 |
| Hand effort to lift full working load ( kg ) | | 30 |
| Load chain | Diameter ( mm ) | 4.0 |
| No. of falls | 1 |
| Grade of chain | V |
| Net weight ( kg ) | | 2.0 |